**Case1: a 8.8 Hz self-excited mode caused by deliberately detuned IBR current loop: DEF is effective**

A screenshot of a graph

Description automatically generated

****

**A group of graphs with lines

Description automatically generated with medium confidence**

**Case 2: a 1.5 Hz self-excited mode caused by high power output of IBR with low system strength: DEF fails**

**A screenshot of a graph

Description automatically generated**

****

**A group of graphs with different colored lines

Description automatically generated**

**Case 3： a 7-bus system with 1 SG (bus 5) and 5 IBR( bus 3,4,5,6,7). 18.76Hz Oscillation caused by badly tuned voltage control of A4 and A7 (A7 worst)**

A screenshot of a graph

Description automatically generated



**A group of blue bars

Description automatically generated**

**A group of lines with numbers

Description automatically generated with medium confidence**